**Nimbus 3(ArjoHuntleigh) -changing the mattress onto transport mode**



|  |
| --- |
|  |

Advice Sheet No. 6

In the event of a power cut follow the directions below to change the mattress into transport mode (static mode)

To transport a patient using the ***Nimbus* 3** turn the transport control at the foot end of the mattress clockwise to **Transport** (See Figure 1). Switch off the pump and disconnect the tube set. To resume normal operation, reconnect the pump, turn the transport control counter-clockwise to **Normal** (See Figure 2) and switch on.

Figure 1Figure 2

Make sure the mattress tube set is not "kinked" or twisted and connect it to the pump until it clicks into place. Make sure the tube set is securely connected to the pump and the mattress.



*Some of the older Nimbus Systems may have the old style tube set. If this is the case DO NOT fit as above. Instead see below.*



In transport mode the mattress will remain inflated for up to 12 hours depending on the patients’ weight.

The Nimbus 3 has audible and visual power fail alarm system.

REFERENCES

Taken from ArjoHuntleigh Nimbus 3 quick reference guide.